**13P1 Hook Panel Specifications**

**PART 1 - GENERAL**

1. DESCRIPTION: Furnish and install wall mounted hook panels.
2. RELATED WORK: (Refer to Section of Specs which applies to wall blocking.)

**PART 2 - PRODUCTS**

1. MANUFACTURER: 13P1series hook panel by EMCO Specialty Products, Inc., Kansas City, KS.
2. MATERIALS: Panel shall be of solid (walnut or oak) 5/8”x 5 5/8”x 17” hardwood and drilled for standard number of hooks. The finish is to be (specify walnut, medium oak, or light oak).
3. 13P1 panels shall have two P1 hooks (specify finish either silver or black) and one D10 slotted hook to accommodate one hanger. All hooks to be installed at the factory.
4. ACCESSORIES: One EMCO hanger No.13 ball top hanger shall be provided for the in the center hook. Hanger to match panel finish.

**PART 3 - EXECUTION**

INSTALLATION:

* 1. Install wall blocking.
	2. Install concealed fastener mounting plate to wall using “fasteners by others” appropriate for wall type.
	3. Install panel at height specified by architect.
	4. Check to make sure it is level.
	5. Remove adhesive backing strip from back of panel.
	6. Slide panel concealed fastener over wall mounting plate.
	7. Install hanger in hook slot.
	8. Wipe down panel to remove dust.
	9. Remove all trash and debris.