**W Hook Strip Specifications**

**PART 1 - GENERAL**

1. DESCRIPTION: Furnish and install custom length wall mounted hook strip.
2. RELATED WORK: (Refer to Section of Specs which applies to wall blocking for coat racks.)

**PART 2 - PRODUCTS**

1. MANUFACTURER: W Hook Strip unit by EMCO Specialty Products, Inc., Kansas City, KS.
2. MATERIALS:
	1. Wall strips are 1/2" extruded aluminum 6” long, powder coated black.
	2. Brackets are solid cast aluminum powder coated black. Bracket screws are included to allow for height adjustment.
	3. Shelf slat is extruded aluminum (specify finish either silver or bronze).
	4. Hook Strip shall include double-pronged polycarbonate 10HK hook locked in place. The number and arrangement as per manufacturer's standards. Hook color to be (specify black, blue, brown, gray, green, orange, purple, red, yellow, or assorted colors.)

**PART 3 - EXECUTION**

INSTALLATION:

* 1. Install wall blocking.
	2. Install wall strip using “fasteners by others” appropriate for wall type.
	3. The wall strip height shall be based upon architect’s specified height for unit.
	4. Install brackets in wall strip using EMCO fasteners.
	5. Install slat using EMCO fasteners.
	6. Wipe down shelves to remove dust.
	7. Remove all trash and debris.