**#33 Coat Rack Specifications**

**PART 1 - GENERAL**

1. DESCRIPTION: Furnish and install custom length wall mounted coat rack.
2. RELATED WORK: (Refer to Section of Specs which applies to wall blocking for coat racks.)

**PART 2 - PRODUCTS**

1. MANUFACTURER: #33 unit by EMCO Specialty Products, Inc., Kansas City, KS.
2. MATERIALS:
   1. Brackets are solid cast aluminum powder coated black. Bracket screws are included to allow for height adjustment.
   2. Shelf slat is extruded aluminum (specify finish either silver or bronze).
   3. #33 shall include double-pronged polycarbonate 10HK hook locked in place in second and forth slat. The number and arrangement as per manufacturer's standards. Hook color to be (specify black, blue, brown, gray, green, orange, purple, red, yellow, or assorted colors.)

**PART 3 - EXECUTION**

INSTALLATION:

* 1. Install wall blocking.
  2. Install bracket using “fasteners by others” appropriate for wall type.
  3. The bracket height shall be based upon architect’s specified shelf height.
  4. Install slat using EMCO fasteners.
  5. Wipe down shelves to remove dust.
  6. Remove all trash and debris.