**L1 Hook Specifications**

**PART 1 - GENERAL**

1. DESCRIPTION: Furnish and install wall mounted hooks.
2. RELATED WORK: (Refer to Section of Specs which applies to wall blocking.)

**PART 2 - PRODUCTS**

1. MANUFACTURER: L1 hook by EMCO Specialty Products, Inc., Kansas City, KS.
2. MATERIALS: Hook shall be of solid aluminum 2” high, 1 3/8” wide and projecting 2 5/8” from the wall. The finish is to be anodized aluminum. Color to be silver.

**PART 3 - EXECUTION**

INSTALLATION:

* 1. Install wall blocking.
	2. Install hook using manufacturer’s fasteners if appropriate for wall type. (Screws provided by EMCO are not intended for all wall types.)
	3. Install hook at height & location specified by architect.
	4. Wipe down hook to remove dust.
	5. Remove all trash and debris.